# Scheduled WAN Disconnect - MikroTik Script RouterOS

    "t-dsl" is the name of the WAN-interface, PPPoE in this case

    / system scheduler
    add name="sched_disconnect" on-event=pppoe_dis start-date=jan/01/2006 start-time=03:00:00 interval=1d \
    comment="move daily T-DSL-disconnect to late night" disabled=yes

    /system script
    add name=pppoe_dis source={/interface pppoe-client disable [find name="t-dsl"]
    :delay 10
    /interface pppoe-client enable [find name="t-dsl"]
    :log info "Script pppoe_dis - scheduled T-DSL-disconnect executed."
    }
    should be tested in your environment and use it by own risk!

    ....or simply name your pppoe interface "ADSL" and do it within scheduler without scripting ...

    /system scheduler
    add  name="ADSL reconect" interval=1d on-event="interface pppoe-client disable ADSL ;\r\
    interface pppoe-client enable ADSL ;\r\
    " policy=ftp,reboot,read,write,policy,test,winbox,password,sniff,sensitive,a
    start-date=sep/12/2012 start-time=06:00:00
    Credit: wiki.mikrotik.com