# How to Setting Bonding Interface - MikroTik Script RouterOS

    Bonding is a technology that allows the aggregation of several Ethernet interfaces into one virtual link, so that it can get a higher data rate/bandwidth and can become a failover link.

    # ROUTER 1
    # ========
    /interface bonding
    add slaves=ether4,ether5 disabled=no
    /ip address
    add address=192.168.50.1/24 interface=bonding1

    # ROUTER 2
    # ========
    /interface bonding
    add slaves=ether4,ether5 disabled=no
    /ip address
    add address=192.168.50.2/24 interface=bonding1
    Credit: o-om.com