# IP Private or IP Local Standard RFC 1918 - Mikrotik Script RouterOS

    Address Allocation for Private Internets
    This document specifies an Internet Best Current Practices for the
    Internet Community, and requests discussion and suggestions for
    improvements.  Distribution of this memo is unlimited.

    read more > Address Allocation for Private Internet

    /ip firewall address-list
    add address=0.0.0.0/8 list=LOCAL-IP
    add address=10.0.0.0/8 list=LOCAL-IP
    add address=100.64.0.0/10 list=LOCAL-IP
    add address=127.0.0.0/8 list=LOCAL-IP
    add address=169.254.0.0/16 list=LOCAL-IP
    add address=172.16.0.0/12 list=LOCAL-IP
    add address=192.0.0.0/24 list=LOCAL-IP
    add address=192.0.2.0/24 list=LOCAL-IP
    add address=192.168.0.0/16 list=LOCAL-IP
    add address=198.18.0.0/15 list=LOCAL-IP
    add address=198.51.100.0/24 list=LOCAL-IP
    add address=203.0.113.0/24 list=LOCAL-IP
    add address=224.0.0.0/4 list=LOCAL-IP
    add address=240.0.0.0/4 list=LOCAL-IP
    Credit: https://tools.ietf.org/html/rfc1918