# Change Name Interface or Ether To Default Manua - Mikrotik Script RouterOS

    I made this simple script to make it easier for us to return the interface name (ether) to the factory default name without having to reset the proxy. There are times when we forget the order on the Mikrotik port even though we have given the ether name, for example with the name "LAN" but whether "LAN" is plugged into what port. so the meaning is clear :)

    #####################################
    # Script by Agus Ramadhani
    # fb.com/buananet.pangkalanbun
    # http://www.o-om.com
    # SCRIPT name interface to default
    ######################################
    /interface ethernet
    set [ find default-name=ether1 ] name=ether1
    set [ find default-name=ether2 ] name=ether2
    set [ find default-name=ether3 ] name=ether3
    set [ find default-name=ether4 ] name=ether4
    set [ find default-name=ether5 ] name=ether5
    set [ find default-name=ether6 ] name=ether6
    set [ find default-name=ether7 ] name=ether7
    set [ find default-name=ether8 ] name=ether8
    set [ find default-name=ether9 ] name=ether9
    set [ find default-name=ether10 ] name=ether10
    set [ find default-name=ether11 ] name=ether11
    set [ find default-name=ether12 ] name=ether12
    set [ find default-name=ether13 ] name=ether13
    set [ find default-name=combo1 ] name=combo1
    set [ find default-name=combo2 ] name=combo2
    set [ find default-name=wlan1 ] name=wlan1
    set [ find default-name=wlan2 ] name=wlan2
    set [ find default-name=sfp1 ] name=sfp1
    set [ find default-name=sfp2 ] name=sfp2
    set [ find default-name=sfp3 ] name=sfp3
    set [ find default-name=sfp4 ] name=sfp4
    set [ find default-name=sfp-sfpplus1 ] name=sfp-sfpplus1
    set [ find default-name=sfp-sfpplus2 ] name=sfp-sfpplus2
    Credit: www.o-om.com