# Mikrotik Port Service FTP 21 - MikroTik Script RouterOS

    Mikrotik provides a standard FTP service that uses ports 20 and 21. FTP is usually used to upload or download router data, such as backup files. FTP authorization using router account user & password. This FTP port is often attacked using BRUTE FORCE, you can change the port or disable it when not in use.

    # FTP Port Enable
    /ip service set ftp port=21 address=0.0.0.0/0 disabled=no
    # FTP Port Disable
    /ip service set ftp port=21 address=0.0.0.0/0 disabled=yes
    Credit: mikrotik.co.id