# Change MAC Address From Terminal - MikroTik Script RouterOS

    By default changing MAC address of ethernet interface in Mikrotik Winbox is disabled:

    But You can very simple change MAC in terminal.

    In left side menu select New Terminal:

    /interface ethernet set ether1 mac-address=XX:XX:XX:XX:XX:XX
    Where ether1 is required interface and XX:XX:XX:XX:XX:XX is new MAC address of your device.

    Credit: https://andjey.info/how-to-change-mac-address-on-mikrotik-routerboard/