# Backup Use Import rsc - Mikrotik Script RouterOS

    To import the exported file is quite easy

    /import file=[filename]
    However, the results of imports with different routers will usually experience problems or maybe because of duplication of existing files,
    to solve this problem try using the verbose = yes command, at least by verbose we can find out where and what line the error is located.

    /import file=[filename] verbose=yes
    Credit: www.o-om.com