# Mikrotik Port Service WWW 80 Webfig - MikroTik Script RouterOS

    In addition to the remote console and winbox, Mikrotik also provides a way to access the router via a web-base using a browser. The port used is the standard HTTP port, which is port 80, You can change the port or disable it when not in use.

    # WWW (webfig) Port Enable
    /ip service set www port=80 address=0.0.0.0/0 disabled=no
    # WWW (webfig) Port Disable
    /ip service set www port=80 address=0.0.0.0/0 disabled=yes
    Credit: mikrotik.co.id