# Mikrotik Port Service WINBOX 8291 - MikroTik Script RouterOS

    The service that allows the Winbox application to connect to the router. Of course we are already familiar with the Winbox application which is used to graphically remotely router. Winbox connection using port 8291. Some versions of routeros can be hacked using an exploit, You can change the Port for more Secure!

    # WINBOX Port Enable
    /ip service set winbox port=8291 address=0.0.0.0/0 disabled=no
    # WINBOX Port Disable
    /ip service set winbox port=8291 address=0.0.0.0/0 disabled=yes
    Credit: mikrotik.co.id